#MicroXplorer Configuration settings - do not modify
CORTEX_M7.ART_ACCLERATOR_ENABLE=1
CORTEX_M7.AccessPermission-Cortex_Memory_Protection_Unit_Region0_Settings=MPU_REGION_FULL_ACCESS
CORTEX_M7.AccessPermission-Cortex_Memory_Protection_Unit_Region1_Settings=MPU_REGION_FULL_ACCESS
CORTEX_M7.BaseAddress-Cortex_Memory_Protection_Unit_Region0_Settings=0x90000000
CORTEX_M7.BaseAddress-Cortex_Memory_Protection_Unit_Region1_Settings=0x90000000
CORTEX_M7.CPU_DCache=Enabled
CORTEX_M7.CPU_ICache=Enabled
CORTEX_M7.Enable-Cortex_Memory_Protection_Unit_Region0_Settings=MPU_REGION_ENABLE
CORTEX_M7.Enable-Cortex_Memory_Protection_Unit_Region1_Settings=MPU_REGION_ENABLE
CORTEX_M7.IPParameters=CPU_ICache,CPU_DCache,ART_ACCLERATOR_ENABLE,PREFETCH_ENABLE,MPU_Control,Enable-Cortex_Memory_Protection_Unit_Region0_Settings,BaseAddress-Cortex_Memory_Protection_Unit_Region0_Settings,Size-Cortex_Memory_Protection_Unit_Region0_Settings,AccessPermission-Cortex_Memory_Protection_Unit_Region0_Settings,Enable-Cortex_Memory_Protection_Unit_Region1_Settings,BaseAddress-Cortex_Memory_Protection_Unit_Region1_Settings,Size-Cortex_Memory_Protection_Unit_Region1_Settings,AccessPermission-Cortex_Memory_Protection_Unit_Region1_Settings,IsCacheable-Cortex_Memory_Protection_Unit_Region1_Settings
CORTEX_M7.IsCacheable-Cortex_Memory_Protection_Unit_Region1_Settings=MPU_ACCESS_CACHEABLE
CORTEX_M7.MPU_Control=MPU_PRIVILEGED_DEFAULT
CORTEX_M7.PREFETCH_ENABLE=1
CORTEX_M7.Size-Cortex_Memory_Protection_Unit_Region0_Settings=MPU_REGION_SIZE_256MB
CORTEX_M7.Size-Cortex_Memory_Protection_Unit_Region1_Settings=MPU_REGION_SIZE_16MB
FMC.CASLatency1=FMC_SDRAM_CAS_LATENCY_3
FMC.ExitSelfRefreshDelay1=7
FMC.IPParameters=CASLatency1,SDClockPeriod1,SDClockPeriod2,ReadBurst1,ReadBurst2,LoadToActiveDelay1,ExitSelfRefreshDelay1,SelfRefreshTime1,RowCycleDelay1,RowCycleDelay2,WriteRecoveryTime1,RPDelay1,RPDelay2,RCDDelay1
FMC.LoadToActiveDelay1=2
FMC.RCDDelay1=2
FMC.RPDelay1=2
FMC.RPDelay2=2
FMC.ReadBurst1=FMC_SDRAM_RBURST_ENABLE
FMC.ReadBurst2=FMC_SDRAM_RBURST_ENABLE
FMC.RowCycleDelay1=7
FMC.RowCycleDelay2=7
FMC.SDClockPeriod1=FMC_SDRAM_CLOCK_PERIOD_2
FMC.SDClockPeriod2=FMC_SDRAM_CLOCK_PERIOD_2
FMC.SelfRefreshTime1=4
FMC.WriteRecoveryTime1=3
FREERTOS.FootprintOK=true
FREERTOS.IPParameters=Tasks01,configUSE_APPLICATION_TASK_TAG,configUSE_RECURSIVE_MUTEXES,configUSE_COUNTING_SEMAPHORES,configUSE_IDLE_HOOK,configUSE_MALLOC_FAILED_HOOK,configCHECK_FOR_STACK_OVERFLOW,configTOTAL_HEAP_SIZE,MEMORY_ALLOCATION,FootprintOK
FREERTOS.MEMORY_ALLOCATION=0
FREERTOS.Tasks01=defaultTaskHand,0,4096,StartDefaultTask,Default,NULL,Dynamic,NULL,NULL
FREERTOS.configCHECK_FOR_STACK_OVERFLOW=2
FREERTOS.configTOTAL_HEAP_SIZE=32768
FREERTOS.configUSE_APPLICATION_TASK_TAG=1
FREERTOS.configUSE_COUNTING_SEMAPHORES=1
FREERTOS.configUSE_IDLE_HOOK=1
FREERTOS.configUSE_MALLOC_FAILED_HOOK=1
FREERTOS.configUSE_RECURSIVE_MUTEXES=1
File.Version=6
GPIO.groupedBy=Group By Peripherals
I2C3.I2C_Rise_Time=0
I2C3.IPParameters=Timing,Speed,I2C_Rise_Time
I2C3.Speed=100
I2C3.Timing=0x00C0EAFF
KeepUserPlacement=true
LTDC.ActiveH=272
LTDC.ActiveW=480
LTDC.Alpha_L0=255
LTDC.BlendingFactor1_L0=LTDC_BLENDING_FACTOR1_CA
LTDC.BlendingFactor2_L0=LTDC_BLENDING_FACTOR2_CA
LTDC.FBStartAdress_L0=0xC0000000
LTDC.Green_L0=0
LTDC.HBP=13
LTDC.HFP=32
LTDC.HSync=41
LTDC.IPParameters=ActiveW,ActiveH,HSync,HBP,HFP,VSync,Layers,WindowX1_L0,WindowY1_L0,Alpha_L0,BlendingFactor1_L0,BlendingFactor2_L0,FBStartAdress_L0,ImageWidth_L0,PixelFormat_L0,ImageHeight_L0,Green_L0
LTDC.ImageHeight_L0=272
LTDC.ImageWidth_L0=480
LTDC.Layers=0
LTDC.PixelFormat_L0=LTDC_PIXEL_FORMAT_RGB565
LTDC.VSync=10
LTDC.WindowX1_L0=480
LTDC.WindowY1_L0=272
Mcu.Family=STM32F7
Mcu.IP0=CORTEX_M7
Mcu.IP1=CRC
Mcu.IP10=SYS
Mcu.IP2=DMA2D
Mcu.IP3=FMC
Mcu.IP4=FREERTOS
Mcu.IP5=I2C3
Mcu.IP6=LTDC
Mcu.IP7=NVIC
Mcu.IP8=QUADSPI
Mcu.IP9=RCC
Mcu.IPNb=11
Mcu.Name=STM32F746NGHx
Mcu.Package=TFBGA216
Mcu.Pin0=PE4
Mcu.Pin1=PE3
Mcu.Pin10=PD7
Mcu.Pin100=PD15
Mcu.Pin101=PB13
Mcu.Pin102=PD10
Mcu.Pin103=PF10
Mcu.Pin104=PF9
Mcu.Pin105=PF8
Mcu.Pin106=PC3
Mcu.Pin107=PD14
Mcu.Pin108=PB12
Mcu.Pin109=PD9
Mcu.Pin11=PC12
Mcu.Pin110=PD8
Mcu.Pin111=PC0
Mcu.Pin112=PC1
Mcu.Pin113=PC2
Mcu.Pin114=PB2
Mcu.Pin115=PF12
Mcu.Pin116=PG1
Mcu.Pin117=PF15
Mcu.Pin118=PJ4
Mcu.Pin119=PD12
Mcu.Pin12=PA15
Mcu.Pin120=PD13
Mcu.Pin121=PG3
Mcu.Pin122=PG2
Mcu.Pin123=PJ5
Mcu.Pin124=PH12
Mcu.Pin125=PA1
Mcu.Pin126=PA0/WKUP
Mcu.Pin127=PA4
Mcu.Pin128=PC4
Mcu.Pin129=PF13
Mcu.Pin13=PA14
Mcu.Pin130=PG0
Mcu.Pin131=PJ3
Mcu.Pin132=PE8
Mcu.Pin133=PD11
Mcu.Pin134=PG5
Mcu.Pin135=PG4
Mcu.Pin136=PH7
Mcu.Pin137=PH9
Mcu.Pin138=PH11
Mcu.Pin139=PA2
Mcu.Pin14=PA13
Mcu.Pin140=PA6
Mcu.Pin141=PA5
Mcu.Pin142=PC5
Mcu.Pin143=PF14
Mcu.Pin144=PJ2
Mcu.Pin145=PF11
Mcu.Pin146=PE9
Mcu.Pin147=PE11
Mcu.Pin148=PE14
Mcu.Pin149=PB10
Mcu.Pin15=PE5
Mcu.Pin150=PH6
Mcu.Pin151=PH8
Mcu.Pin152=PH10
Mcu.Pin153=PA3
Mcu.Pin154=PA7
Mcu.Pin155=PB1
Mcu.Pin156=PB0
Mcu.Pin157=PJ0
Mcu.Pin158=PJ1
Mcu.Pin159=PE7
Mcu.Pin16=PE6
Mcu.Pin160=PE10
Mcu.Pin161=PE12
Mcu.Pin162=PE15
Mcu.Pin163=PE13
Mcu.Pin164=PB11
Mcu.Pin165=PB14
Mcu.Pin166=PB15
Mcu.Pin167=VP_CRC_VS_CRC
Mcu.Pin168=VP_DMA2D_VS_DMA2D
Mcu.Pin169=VP_FREERTOS_VS_CMSIS_V1
Mcu.Pin17=PG13
Mcu.Pin170=VP_SYS_VS_tim6
Mcu.Pin171=VP_STMicroelectronics.X-CUBE-TOUCHGFX_VS_GraphicsJjApplication_4.13.0
Mcu.Pin18=PB9
Mcu.Pin19=PB7
Mcu.Pin2=PE2
Mcu.Pin20=PB6
Mcu.Pin21=PG15
Mcu.Pin22=PG11
Mcu.Pin23=PJ13
Mcu.Pin24=PJ12
Mcu.Pin25=PD6
Mcu.Pin26=PD0
Mcu.Pin27=PC11
Mcu.Pin28=PC10
Mcu.Pin29=PA12
Mcu.Pin3=PG14
Mcu.Pin30=PI8
Mcu.Pin31=PI4
Mcu.Pin32=PK7
Mcu.Pin33=PK6
Mcu.Pin34=PK5
Mcu.Pin35=PG12
Mcu.Pin36=PG10
Mcu.Pin37=PJ14
Mcu.Pin38=PD5
Mcu.Pin39=PD3
Mcu.Pin4=PE1
Mcu.Pin40=PD1
Mcu.Pin41=PI3
Mcu.Pin42=PI2
Mcu.Pin43=PA11
Mcu.Pin44=PC13
Mcu.Pin45=PF0
Mcu.Pin46=PI5
Mcu.Pin47=PI7
Mcu.Pin48=PI10
Mcu.Pin49=PI6
Mcu.Pin5=PE0
Mcu.Pin50=PK4
Mcu.Pin51=PK3
Mcu.Pin52=PG9
Mcu.Pin53=PJ15
Mcu.Pin54=PD4
Mcu.Pin55=PD2
Mcu.Pin56=PH15
Mcu.Pin57=PI1
Mcu.Pin58=PA10
Mcu.Pin59=PC14/OSC32_IN
Mcu.Pin6=PB8
Mcu.Pin60=PF1
Mcu.Pin61=PI12
Mcu.Pin62=PI9
Mcu.Pin63=PH13
Mcu.Pin64=PH14
Mcu.Pin65=PI0
Mcu.Pin66=PA9
Mcu.Pin67=PC15/OSC32_OUT
Mcu.Pin68=PK1
Mcu.Pin69=PK2
Mcu.Pin7=PB5
Mcu.Pin70=PC9
Mcu.Pin71=PA8
Mcu.Pin72=PH0/OSC_IN
Mcu.Pin73=PF2
Mcu.Pin74=PI13
Mcu.Pin75=PI15
Mcu.Pin76=PJ11
Mcu.Pin77=PK0
Mcu.Pin78=PC8
Mcu.Pin79=PC7
Mcu.Pin8=PB4
Mcu.Pin80=PH1/OSC_OUT
Mcu.Pin81=PF3
Mcu.Pin82=PI14
Mcu.Pin83=PH4
Mcu.Pin84=PJ8
Mcu.Pin85=PJ10
Mcu.Pin86=PG8
Mcu.Pin87=PC6
Mcu.Pin88=PF4
Mcu.Pin89=PH5
Mcu.Pin9=PB3
Mcu.Pin90=PH3
Mcu.Pin91=PJ7
Mcu.Pin92=PJ9
Mcu.Pin93=PG7
Mcu.Pin94=PG6
Mcu.Pin95=PF7
Mcu.Pin96=PF6
Mcu.Pin97=PF5
Mcu.Pin98=PH2
Mcu.Pin99=PJ6
Mcu.PinsNb=172
Mcu.ThirdParty0=STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0
Mcu.ThirdPartyNb=1
Mcu.UserConstants=
Mcu.UserName=STM32F746NGHx
MxCube.Version=5.6.1
MxDb.Version=DB.5.0.60
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.DMA2D_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.LTDC_IRQn=true\:5\:0\:false\:false\:true\:true\:true\:true
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:false
NVIC.TIM6_DAC_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.TimeBase=TIM6_DAC_IRQn
NVIC.TimeBaseIP=TIM6
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
PA0/WKUP.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_Mode
PA0/WKUP.GPIO_Label=ARDUINO A0
PA0/WKUP.GPIO_Mode=GPIO_MODE_ANALOG
PA0/WKUP.GPIO_PuPd=GPIO_NOPULL
PA0/WKUP.Locked=true
PA0/WKUP.Signal=ADCx_IN0
PA1.GPIOParameters=GPIO_Label
PA1.GPIO_Label=RMII_REF_CLK [LAN8742A-CZ-TR_REFCLK0]
PA1.Locked=true
PA1.Signal=ETH_REF_CLK
PA10.GPIOParameters=GPIO_Label
PA10.GPIO_Label=OTG_FS_ID
PA10.Locked=true
PA10.Signal=USB_OTG_FS_ID
PA11.GPIOParameters=GPIO_Label
PA11.GPIO_Label=OTG_FS_N
PA11.Locked=true
PA11.Signal=USB_OTG_FS_DM
PA12.GPIOParameters=GPIO_Label
PA12.GPIO_Label=OTG_FS_P
PA12.Locked=true
PA12.Signal=USB_OTG_FS_DP
PA13.GPIOParameters=GPIO_Label
PA13.GPIO_Label=SWDIO
PA13.Locked=true
PA13.Mode=Serial_Wire
PA13.Signal=SYS_JTMS-SWDIO
PA14.GPIOParameters=GPIO_Label
PA14.GPIO_Label=SWCLK
PA14.Locked=true
PA14.Mode=Serial_Wire
PA14.Signal=SYS_JTCK-SWCLK
PA15.GPIOParameters=GPIO_ModeDefaultPP,GPIO_Speed,GPIO_PuPd,GPIO_Label
PA15.GPIO_Label=ARDUINO PWM/D9
PA15.GPIO_ModeDefaultPP=GPIO_MODE_AF_PP
PA15.GPIO_PuPd=GPIO_NOPULL
PA15.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PA15.Locked=true
PA15.Signal=S_TIM2_CH1_ETR
PA2.GPIOParameters=GPIO_Label
PA2.GPIO_Label=RMII_MDIO [LAN8742A-CZ-TR_MDIO]
PA2.Locked=true
PA2.Signal=ETH_MDIO
PA3.GPIOParameters=GPIO_Label
PA3.GPIO_Label=ULPI_D0 [USB3320C-EZK_D0]
PA3.Locked=true
PA3.Mode=Host_HS
PA3.Signal=USB_OTG_HS_ULPI_D0
PA4.GPIOParameters=GPIO_Label
PA4.GPIO_Label=DCMI_HSYNC
PA4.Locked=true
PA4.Signal=DCMI_HSYNC
PA5.GPIOParameters=GPIO_Label
PA5.GPIO_Label=ULPI_CLK [USB3320C-EZK_CLKOUT]
PA5.Locked=true
PA5.Mode=Host_HS
PA5.Signal=USB_OTG_HS_ULPI_CK
PA6.Locked=true
PA6.Signal=DCMI_PIXCLK
PA7.GPIOParameters=GPIO_Label
PA7.GPIO_Label=RMII_CRS_DV [LAN8742A-CZ-TR_CRS_DV]
PA7.Locked=true
PA7.Signal=ETH_CRS_DV
PA8.GPIOParameters=GPIO_ModeDefaultPP,GPIO_Speed,GPIO_PuPd,GPIO_Label
PA8.GPIO_Label=ARDUINO PWM/D10
PA8.GPIO_ModeDefaultPP=GPIO_MODE_AF_PP
PA8.GPIO_PuPd=GPIO_NOPULL
PA8.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PA8.Locked=true
PA8.Signal=S_TIM1_CH1
PA9.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PA9.GPIO_Label=VCP_TX [STM32F103CBT6_PA3]
PA9.GPIO_Mode=GPIO_MODE_AF_PP
PA9.GPIO_PuPd=GPIO_NOPULL
PA9.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PA9.Locked=true
PA9.Signal=USART1_TX
PB0.GPIOParameters=GPIO_Label
PB0.GPIO_Label=ULPI_D1 [USB3320C-EZK_D1]
PB0.Locked=true
PB0.Mode=Host_HS
PB0.Signal=USB_OTG_HS_ULPI_D1
PB1.GPIOParameters=GPIO_Label
PB1.GPIO_Label=ULPI_D2 [USB3320C-EZK_D2]
PB1.Locked=true
PB1.Mode=Host_HS
PB1.Signal=USB_OTG_HS_ULPI_D2
PB10.GPIOParameters=GPIO_Label
PB10.GPIO_Label=ULPI_D3 [USB3320C-EZK_D3]
PB10.Locked=true
PB10.Signal=USB_OTG_HS_ULPI_D3
PB11.GPIOParameters=GPIO_Label
PB11.GPIO_Label=ULPI_D4 [USB3320C-EZK_D4]
PB11.Locked=true
PB11.Mode=Host_HS
PB11.Signal=USB_OTG_HS_ULPI_D4
PB12.GPIOParameters=GPIO_Label
PB12.GPIO_Label=ULPI_D5 [USB3320C-EZK_D5]
PB12.Locked=true
PB12.Mode=Host_HS
PB12.Signal=USB_OTG_HS_ULPI_D5
PB13.GPIOParameters=GPIO_Label
PB13.GPIO_Label=ULPI_D6 [USB3320C-EZK_D6]
PB13.Locked=true
PB13.Mode=Host_HS
PB13.Signal=USB_OTG_HS_ULPI_D6
PB14.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PB14.GPIO_Label=ARDUINO MISO/D12
PB14.GPIO_Mode=GPIO_MODE_AF_PP
PB14.GPIO_PuPd=GPIO_NOPULL
PB14.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB14.Locked=true
PB14.Signal=SPI2_MISO
PB15.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PB15.GPIO_Label=ARDUINO MOSI/PWM/D11
PB15.GPIO_Mode=GPIO_MODE_AF_PP
PB15.GPIO_PuPd=GPIO_NOPULL
PB15.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB15.Locked=true
PB15.Signal=SPI2_MOSI
PB2.Locked=true
PB2.Mode=Single Bank 1
PB2.Signal=QUADSPI_CLK
PB3.GPIOParameters=GPIO_Label
PB3.GPIO_Label=SWO
PB3.Locked=true
PB3.Signal=SYS_JTDO-SWO
PB4.GPIOParameters=GPIO_ModeDefaultPP,GPIO_Speed,GPIO_PuPd,GPIO_Label
PB4.GPIO_Label=ARDUINO PWM/D3
PB4.GPIO_ModeDefaultPP=GPIO_MODE_AF_PP
PB4.GPIO_PuPd=GPIO_NOPULL
PB4.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB4.Locked=true
PB4.Signal=S_TIM3_CH1
PB5.GPIOParameters=GPIO_Label
PB5.GPIO_Label=ULPI_D7 [USB3320C-EZK_D7]
PB5.Locked=true
PB5.Mode=Host_HS
PB5.Signal=USB_OTG_HS_ULPI_D7
PB6.GPIOParameters=GPIO_Label
PB6.GPIO_Label=QSPI_NCS [N25Q128A13EF840E_S]
PB6.Locked=true
PB6.Mode=Single Bank 1
PB6.Signal=QUADSPI_BK1_NCS
PB7.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PB7.GPIO_Label=VCP_RX [STM32F103CBT6_PA2]
PB7.GPIO_Mode=GPIO_MODE_AF_PP
PB7.GPIO_PuPd=GPIO_NOPULL
PB7.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB7.Locked=true
PB7.Signal=USART1_RX
PB8.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PB8.GPIO_Label=ARDUINO SCL/D15
PB8.GPIO_Mode=GPIO_MODE_AF_OD
PB8.GPIO_PuPd=GPIO_NOPULL
PB8.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB8.Locked=true
PB8.Signal=I2C1_SCL
PB9.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PB9.GPIO_Label=ARDUINO SDA/D14
PB9.GPIO_Mode=GPIO_MODE_AF_OD
PB9.GPIO_PuPd=GPIO_NOPULL
PB9.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PB9.Locked=true
PB9.Signal=I2C1_SDA
PC0.GPIOParameters=GPIO_Label
PC0.GPIO_Label=ULPI_STP [USB3320C-EZK_STP]
PC0.Locked=true
PC0.Mode=Host_HS
PC0.Signal=USB_OTG_HS_ULPI_STP
PC1.GPIOParameters=GPIO_Label
PC1.GPIO_Label=RMII_MDC [LAN8742A-CZ-TR_MDC]
PC1.Locked=true
PC1.Signal=ETH_MDC
PC10.GPIOParameters=GPIO_Label
PC10.GPIO_Label=SDMMC_D2
PC10.Locked=true
PC10.Signal=SDMMC1_D2
PC11.GPIOParameters=GPIO_Label
PC11.GPIO_Label=SDMMC_D3
PC11.Locked=true
PC11.Signal=SDMMC1_D3
PC12.GPIOParameters=GPIO_Label
PC12.GPIO_Label=SDMMC_CK
PC12.Locked=true
PC12.Signal=SDMMC1_CK
PC13.GPIOParameters=GPIO_Label
PC13.GPIO_Label=uSD_Detect
PC13.Locked=true
PC13.Signal=GPIO_Input
PC14/OSC32_IN.GPIOParameters=GPIO_Label
PC14/OSC32_IN.GPIO_Label=RCC_OSC32_IN
PC14/OSC32_IN.Locked=true
PC14/OSC32_IN.Signal=RCC_OSC32_IN
PC15/OSC32_OUT.GPIOParameters=GPIO_Label
PC15/OSC32_OUT.GPIO_Label=RCC_OSC32_OUT
PC15/OSC32_OUT.Locked=true
PC15/OSC32_OUT.Signal=RCC_OSC32_OUT
PC2.GPIOParameters=GPIO_Label
PC2.GPIO_Label=ULPI_DIR [USB3320C-EZK_DIR]
PC2.Locked=true
PC2.Mode=Host_HS
PC2.Signal=USB_OTG_HS_ULPI_DIR
PC3.GPIOParameters=GPIO_Label
PC3.GPIO_Label=FMC_SDCKE0 [MT48LC4M32B2B5-6A_CKE]
PC3.Locked=true
PC3.Mode=SdramChipSelect1_1
PC3.Signal=FMC_SDCKE0
PC4.GPIOParameters=GPIO_Label
PC4.GPIO_Label=RMII_RXD0 [LAN8742A-CZ-TR_RXD0]
PC4.Locked=true
PC4.Signal=ETH_RXD0
PC5.GPIOParameters=GPIO_Label
PC5.GPIO_Label=RMII_RXD1 [LAN8742A-CZ-TR_RXD1]
PC5.Locked=true
PC5.Signal=ETH_RXD1
PC6.GPIOParameters=GPIO_Label
PC6.GPIO_Label=ARDUINO TX/D1
PC6.Locked=true
PC6.Signal=USART6_TX
PC7.GPIOParameters=GPIO_Label
PC7.GPIO_Label=ARDUINO RX/D0
PC7.Locked=true
PC7.Signal=USART6_RX
PC8.Locked=true
PC8.Signal=SDMMC1_D0
PC9.Locked=true
PC9.Signal=SDMMC1_D1
PD0.GPIOParameters=GPIO_Label
PD0.GPIO_Label=FMC_D2 [MT48LC4M32B2B5-6A_DQ2]
PD0.Locked=true
PD0.Signal=FMC_D2_DA2
PD1.GPIOParameters=GPIO_Label
PD1.GPIO_Label=FMC_D3 [MT48LC4M32B2B5-6A_DQ3]
PD1.Locked=true
PD1.Signal=FMC_D3_DA3
PD10.GPIOParameters=GPIO_Label
PD10.GPIO_Label=FMC_D15 [MT48LC4M32B2B5-6A_DQ15]
PD10.Locked=true
PD10.Signal=FMC_D15_DA15
PD11.GPIOParameters=GPIO_Label
PD11.GPIO_Label=QSPI_D0 [N25Q128A13EF840E_DQ0]
PD11.Locked=true
PD11.Mode=Single Bank 1
PD11.Signal=QUADSPI_BK1_IO0
PD12.GPIOParameters=GPIO_Label
PD12.GPIO_Label=QSPI_D1 [N25Q128A13EF840E_DQ1]
PD12.Locked=true
PD12.Mode=Single Bank 1
PD12.Signal=QUADSPI_BK1_IO1
PD13.GPIOParameters=GPIO_Label
PD13.GPIO_Label=QSPI_D3 [N25Q128A13EF840E_DQ3]
PD13.Locked=true
PD13.Mode=Single Bank 1
PD13.Signal=QUADSPI_BK1_IO3
PD14.GPIOParameters=GPIO_Label
PD14.GPIO_Label=FMC_D0 [MT48LC4M32B2B5-6A_DQ0]
PD14.Locked=true
PD14.Signal=FMC_D0_DA0
PD15.GPIOParameters=GPIO_Label
PD15.GPIO_Label=FMC_D1 [MT48LC4M32B2B5-6A_DQ1]
PD15.Locked=true
PD15.Signal=FMC_D1_DA1
PD2.GPIOParameters=GPIO_Label
PD2.GPIO_Label=SDMMC_CMD
PD2.Locked=true
PD2.Signal=SDMMC1_CMD
PD3.GPIOParameters=GPIO_Label
PD3.GPIO_Label=DCMI_D5
PD3.Locked=true
PD3.Signal=DCMI_D5
PD4.GPIOParameters=GPIO_Label
PD4.GPIO_Label=OTG_FS_OverCurrent [STMPS2141STR_Fault]
PD4.Locked=true
PD4.Signal=GPIO_Input
PD5.GPIOParameters=PinState,GPIO_Label
PD5.GPIO_Label=OTG_FS_PowerSwitchOn [STMPS2141STR_EN]
PD5.Locked=true
PD5.PinState=GPIO_PIN_SET
PD5.Signal=GPIO_Output
PD6.GPIOParameters=GPIO_Label,GPIO_ModeDefaultEXTI
PD6.GPIO_Label=Audio_INT
PD6.GPIO_ModeDefaultEXTI=GPIO_MODE_EVT_RISING
PD6.Locked=true
PD6.Signal=GPXTI6
PD7.GPIOParameters=GPIO_Label
PD7.GPIO_Label=SPDIF_RX0 [74LVC1G04SE_4]
PD7.Locked=true
PD7.Signal=SPDIFRX_IN0
PD8.GPIOParameters=GPIO_Label
PD8.GPIO_Label=FMC_D13 [MT48LC4M32B2B5-6A_DQ13]
PD8.Locked=true
PD8.Signal=FMC_D13_DA13
PD9.GPIOParameters=GPIO_Label
PD9.GPIO_Label=FMC_D14 [MT48LC4M32B2B5-6A_DQ14]
PD9.Locked=true
PD9.Signal=FMC_D14_DA14
PE0.GPIOParameters=GPIO_Label
PE0.GPIO_Label=FMC_NBL0 [MT48LC4M32B2B5-6A_DQM0]
PE0.Locked=true
PE0.Signal=FMC_NBL0
PE1.GPIOParameters=GPIO_Label
PE1.GPIO_Label=FMC_NBL1 [MT48LC4M32B2B5-6A_DQM1]
PE1.Locked=true
PE1.Signal=FMC_NBL1
PE10.GPIOParameters=GPIO_Label
PE10.GPIO_Label=FMC_D7 [MT48LC4M32B2B5-6A_DQ7]
PE10.Locked=true
PE10.Signal=FMC_D7_DA7
PE11.GPIOParameters=GPIO_Label
PE11.GPIO_Label=FMC_D8 [MT48LC4M32B2B5-6A_DQ8]
PE11.Locked=true
PE11.Signal=FMC_D8_DA8
PE12.GPIOParameters=GPIO_Label
PE12.GPIO_Label=FMC_D9 [MT48LC4M32B2B5-6A_DQ9]
PE12.Locked=true
PE12.Signal=FMC_D9_DA9
PE13.GPIOParameters=GPIO_Label
PE13.GPIO_Label=FMC_D10 [MT48LC4M32B2B5-6A_DQ10]
PE13.Locked=true
PE13.Signal=FMC_D10_DA10
PE14.GPIOParameters=GPIO_Label
PE14.GPIO_Label=FMC_D11 [MT48LC4M32B2B5-6A_DQ11]
PE14.Locked=true
PE14.Signal=FMC_D11_DA11
PE15.GPIOParameters=GPIO_Label
PE15.GPIO_Label=FMC_D12 [MT48LC4M32B2B5-6A_DQ12]
PE15.Locked=true
PE15.Signal=FMC_D12_DA12
PE2.GPIOParameters=GPIO_Label
PE2.GPIO_Label=QSPI_D2 [N25Q128A13EF840E_DQ2]
PE2.Locked=true
PE2.Mode=Single Bank 1
PE2.Signal=QUADSPI_BK1_IO2
PE3.GPIOParameters=GPIO_Label
PE3.GPIO_Label=OTG_HS_OverCurrent [STMPS2151STR_FAULT]
PE3.Locked=true
PE3.Signal=GPIO_Input
PE4.GPIOParameters=GPIO_Label
PE4.GPIO_Label=LCD_B0 [RK043FN48H-CT672B_B0]
PE4.Locked=true
PE4.Signal=LTDC_B0
PE5.GPIOParameters=GPIO_Label
PE5.GPIO_Label=DCMI_D6
PE5.Locked=true
PE5.Signal=DCMI_D6
PE6.GPIOParameters=GPIO_Label
PE6.GPIO_Label=DCMI_D7
PE6.Locked=true
PE6.Signal=DCMI_D7
PE7.GPIOParameters=GPIO_Label
PE7.GPIO_Label=FMC_D4 [MT48LC4M32B2B5-6A_DQ4]
PE7.Locked=true
PE7.Signal=FMC_D4_DA4
PE8.GPIOParameters=GPIO_Label
PE8.GPIO_Label=FMC_D5 [MT48LC4M32B2B5-6A_DQ5]
PE8.Locked=true
PE8.Signal=FMC_D5_DA5
PE9.GPIOParameters=GPIO_Label
PE9.GPIO_Label=FMC_D6 [MT48LC4M32B2B5-6A_DQ6]
PE9.Locked=true
PE9.Signal=FMC_D6_DA6
PF0.GPIOParameters=GPIO_Label
PF0.GPIO_Label=FMC_A0 [MT48LC4M32B2B5-6A_A0]
PF0.Locked=true
PF0.Signal=FMC_A0
PF1.GPIOParameters=GPIO_Label
PF1.GPIO_Label=FMC_A1 [MT48LC4M32B2B5-6A_A1]
PF1.Locked=true
PF1.Signal=FMC_A1
PF10.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_Mode
PF10.GPIO_Label=ARDUINO A1
PF10.GPIO_Mode=GPIO_MODE_ANALOG
PF10.GPIO_PuPd=GPIO_NOPULL
PF10.Locked=true
PF10.Signal=ADC3_IN8
PF11.GPIOParameters=GPIO_Label
PF11.GPIO_Label=FMC_SDNRAS [MT48LC4M32B2B5-6A_RAS]
PF11.Locked=true
PF11.Signal=FMC_SDNRAS
PF12.GPIOParameters=GPIO_Label
PF12.GPIO_Label=FMC_A6 [MT48LC4M32B2B5-6A_A6]
PF12.Locked=true
PF12.Signal=FMC_A6
PF13.GPIOParameters=GPIO_Label
PF13.GPIO_Label=FMC_A7 [MT48LC4M32B2B5-6A_A7]
PF13.Locked=true
PF13.Signal=FMC_A7
PF14.GPIOParameters=GPIO_Label
PF14.GPIO_Label=FMC_A8 [MT48LC4M32B2B5-6A_A8]
PF14.Locked=true
PF14.Signal=FMC_A8
PF15.GPIOParameters=GPIO_Label
PF15.GPIO_Label=FMC_A9 [MT48LC4M32B2B5-6A_A9]
PF15.Locked=true
PF15.Signal=FMC_A9
PF2.GPIOParameters=GPIO_Label
PF2.GPIO_Label=FMC_A2 [MT48LC4M32B2B5-6A_A2]
PF2.Locked=true
PF2.Signal=FMC_A2
PF3.GPIOParameters=GPIO_Label
PF3.GPIO_Label=FMC_A3 [MT48LC4M32B2B5-6A_A3]
PF3.Locked=true
PF3.Signal=FMC_A3
PF4.GPIOParameters=GPIO_Label
PF4.GPIO_Label=FMC_A4 [MT48LC4M32B2B5-6A_A4]
PF4.Locked=true
PF4.Signal=FMC_A4
PF5.GPIOParameters=GPIO_Label
PF5.GPIO_Label=FMC_A5 [MT48LC4M32B2B5-6A_A5]
PF5.Locked=true
PF5.Signal=FMC_A5
PF6.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_Mode
PF6.GPIO_Label=ARDUINO A5
PF6.GPIO_Mode=GPIO_MODE_ANALOG
PF6.GPIO_PuPd=GPIO_NOPULL
PF6.Locked=true
PF6.Signal=ADC3_IN4
PF7.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_Mode
PF7.GPIO_Label=ARDUINO A4
PF7.GPIO_Mode=GPIO_MODE_ANALOG
PF7.GPIO_PuPd=GPIO_NOPULL
PF7.Locked=true
PF7.Signal=ADC3_IN5
PF8.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_Mode
PF8.GPIO_Label=ARDUINO A3
PF8.GPIO_Mode=GPIO_MODE_ANALOG
PF8.GPIO_PuPd=GPIO_NOPULL
PF8.Locked=true
PF8.Signal=ADC3_IN6
PF9.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_Mode
PF9.GPIO_Label=ARDUINO A2
PF9.GPIO_Mode=GPIO_MODE_ANALOG
PF9.GPIO_PuPd=GPIO_NOPULL
PF9.Locked=true
PF9.Signal=ADC3_IN7
PG0.GPIOParameters=GPIO_Label
PG0.GPIO_Label=FMC_A10 [MT48LC4M32B2B5-6A_A10]
PG0.Locked=true
PG0.Signal=FMC_A10
PG1.GPIOParameters=GPIO_Label
PG1.GPIO_Label=FMC_A11 [MT48LC4M32B2B5-6A_A11]
PG1.Locked=true
PG1.Signal=FMC_A11
PG10.GPIOParameters=GPIO_Label
PG10.GPIO_Label=SAI2_SDB [WM8994ECS/R_ADCDAT1]
PG10.Locked=true
PG10.Signal=SAI2_SD_B
PG11.GPIOParameters=GPIO_Label
PG11.GPIO_Label=RMII_TX_EN [LAN8742A-CZ-TR_TXEN]
PG11.Locked=true
PG11.Signal=ETH_TX_EN
PG12.GPIOParameters=GPIO_Label
PG12.GPIO_Label=LCD_B4 [RK043FN48H-CT672B_B4]
PG12.Locked=true
PG12.Mode=RGB565
PG12.Signal=LTDC_B4
PG13.GPIOParameters=GPIO_Label
PG13.GPIO_Label=RMII_TXD0 [LAN8742A-CZ-TR_TXD0]
PG13.Locked=true
PG13.Signal=ETH_TXD0
PG14.GPIOParameters=GPIO_Label
PG14.GPIO_Label=RMII_TXD1 [LAN8742A-CZ-TR_TXD1]
PG14.Locked=true
PG14.Signal=ETH_TXD1
PG15.GPIOParameters=GPIO_Label
PG15.GPIO_Label=FMC_SDNCAS [MT48LC4M32B2B5-6A_CAS]
PG15.Locked=true
PG15.Signal=FMC_SDNCAS
PG2.GPIOParameters=GPIO_Label
PG2.GPIO_Label=RMII_RXER
PG2.Locked=true
PG2.Signal=GPIO_Input
PG3.GPIOParameters=GPIO_Label
PG3.GPIO_Label=EXT_RST
PG3.Locked=true
PG3.Signal=GPIO_Output
PG4.GPIOParameters=GPIO_Label
PG4.GPIO_Label=FMC_BA0 [MT48LC4M32B2B5-6A_BA0]
PG4.Locked=true
PG4.Signal=FMC_A14_BA0
PG5.GPIOParameters=GPIO_Label
PG5.GPIO_Label=FMC_BA1 [MT48LC4M32B2B5-6A_BA1]
PG5.Locked=true
PG5.Signal=FMC_A15_BA1
PG6.GPIOParameters=GPIO_Label
PG6.GPIO_Label=ARDUINO D2
PG6.Locked=true
PG6.Signal=GPIO_Output
PG7.GPIOParameters=GPIO_Label
PG7.GPIO_Label=ARDUINO D4
PG7.Locked=true
PG7.Signal=GPIO_Output
PG8.GPIOParameters=GPIO_Label
PG8.GPIO_Label=FMC_SDCLK [MT48LC4M32B2B5-6A_CLK]
PG8.Locked=true
PG8.Signal=FMC_SDCLK
PG9.GPIOParameters=GPIO_Label
PG9.GPIO_Label=DCMI_VSYNC
PG9.Locked=true
PG9.Signal=DCMI_VSYNC
PH0/OSC_IN.GPIOParameters=GPIO_Label
PH0/OSC_IN.GPIO_Label=OSC_25M [NZ2520SB-25.00M_OUT]
PH0/OSC_IN.Locked=true
PH0/OSC_IN.Mode=HSE-External-Oscillator
PH0/OSC_IN.Signal=RCC_OSC_IN
PH1/OSC_OUT.Locked=true
PH1/OSC_OUT.Mode=HSE-External-Oscillator
PH1/OSC_OUT.Signal=RCC_OSC_OUT
PH10.GPIOParameters=GPIO_Label
PH10.GPIO_Label=DCMI_D1
PH10.Locked=true
PH10.Signal=DCMI_D1
PH11.GPIOParameters=GPIO_Label
PH11.GPIO_Label=DCMI_D2
PH11.Locked=true
PH11.Signal=DCMI_D2
PH12.GPIOParameters=GPIO_Label
PH12.GPIO_Label=DCMI_D3
PH12.Locked=true
PH12.Signal=DCMI_D3
PH13.GPIOParameters=GPIO_Label
PH13.GPIO_Label=DCMI_PWR_EN
PH13.Locked=true
PH13.Signal=GPIO_Output
PH14.GPIOParameters=GPIO_Label
PH14.GPIO_Label=DCMI_D4
PH14.Locked=true
PH14.Signal=DCMI_D4
PH15.GPIOParameters=GPIO_Label
PH15.GPIO_Label=TP3
PH15.Locked=true
PH15.Signal=GPIO_Input
PH2.GPIOParameters=GPIO_Label
PH2.GPIO_Label=NC2
PH2.Locked=true
PH2.Signal=GPIO_Input
PH3.GPIOParameters=GPIO_Label
PH3.GPIO_Label=FMC_SDNE0 [MT48LC4M32B2B5-6A_CS]
PH3.Locked=true
PH3.Mode=SdramChipSelect1_1
PH3.Signal=FMC_SDNE0
PH4.GPIOParameters=GPIO_Label
PH4.GPIO_Label=ULPI_NXT [USB3320C-EZK_NXT]
PH4.Locked=true
PH4.Mode=Host_HS
PH4.Signal=USB_OTG_HS_ULPI_NXT
PH5.GPIOParameters=GPIO_Label
PH5.GPIO_Label=FMC_SDNME [MT48LC4M32B2B5-6A_WE]
PH5.Locked=true
PH5.Signal=FMC_SDNWE
PH6.GPIOParameters=GPIO_Label
PH6.GPIO_Label=ARDUINO PWM/D6
PH6.Locked=true
PH6.Signal=S_TIM12_CH1
PH7.GPIOParameters=GPIO_Label
PH7.GPIO_Label=LCD_SCL [RK043FN48H-CT672B_SCL]
PH7.Locked=true
PH7.Mode=I2C
PH7.Signal=I2C3_SCL
PH8.GPIOParameters=GPIO_Label
PH8.GPIO_Label=LCD_SDA [RK043FN48H-CT672B_SDA]
PH8.Locked=true
PH8.Mode=I2C
PH8.Signal=I2C3_SDA
PH9.GPIOParameters=GPIO_Label
PH9.GPIO_Label=DCMI_D0
PH9.Locked=true
PH9.Signal=DCMI_D0
PI0.GPIOParameters=GPIO_ModeDefaultPP,GPIO_Speed,GPIO_PuPd,GPIO_Label
PI0.GPIO_Label=ARDUINO PWM/CS/D5
PI0.GPIO_ModeDefaultPP=GPIO_MODE_AF_PP
PI0.GPIO_PuPd=GPIO_NOPULL
PI0.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PI0.Locked=true
PI0.Signal=S_TIM5_CH4
PI1.GPIOParameters=GPIO_Speed,GPIO_PuPd,GPIO_Label,GPIO_Mode
PI1.GPIO_Label=ARDUINO SCK/D13
PI1.GPIO_Mode=GPIO_MODE_AF_PP
PI1.GPIO_PuPd=GPIO_NOPULL
PI1.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PI1.Locked=true
PI1.Signal=SPI2_SCK
PI10.GPIOParameters=GPIO_Label
PI10.GPIO_Label=LCD_HSYNC [RK043FN48H-CT672B_HSYNC]
PI10.Locked=true
PI10.Mode=RGB565
PI10.Signal=LTDC_HSYNC
PI12.GPIOParameters=PinState,GPIO_Label
PI12.GPIO_Label=LCD_DISP [RK043FN48H-CT672B_DISP]
PI12.Locked=true
PI12.PinState=GPIO_PIN_SET
PI12.Signal=GPIO_Output
PI13.GPIOParameters=GPIO_Label,GPIO_ModeDefaultEXTI
PI13.GPIO_Label=LCD_INT
PI13.GPIO_ModeDefaultEXTI=GPIO_MODE_EVT_RISING
PI13.Locked=true
PI13.Signal=GPXTI13
PI14.GPIOParameters=GPIO_Label
PI14.GPIO_Label=LCD_CLK [RK043FN48H-CT672B_CLK]
PI14.Locked=true
PI14.Mode=RGB565
PI14.Signal=LTDC_CLK
PI15.GPIOParameters=GPIO_Label
PI15.GPIO_Label=LCD_R0 [RK043FN48H-CT672B_R0]
PI15.Locked=true
PI15.Signal=LTDC_R0
PI2.GPIOParameters=GPIO_Label
PI2.GPIO_Label=ARDUINO D8
PI2.Locked=true
PI2.Signal=GPIO_Output
PI3.GPIOParameters=GPIO_Label
PI3.GPIO_Label=ARDUINO D7
PI3.Locked=true
PI3.Signal=GPIO_Output
PI4.GPIOParameters=GPIO_Label
PI4.GPIO_Label=SAI2_MCLKA [WM8994ECS/R_MCLK1]
PI4.Locked=true
PI4.Signal=SAI2_MCLK_A
PI5.GPIOParameters=GPIO_Label
PI5.GPIO_Label=SAI2_SCKA [WM8994ECS/R_BCLK1]
PI5.Locked=true
PI5.Signal=SAI2_SCK_A
PI6.GPIOParameters=GPIO_Label
PI6.GPIO_Label=SAI2_SDA [WM8994ECS/R_DACDAT1]
PI6.Locked=true
PI6.Signal=SAI2_SD_A
PI7.GPIOParameters=GPIO_Label
PI7.GPIO_Label=SAI2_FSA [WM8994ECS/R_LRCLK1]
PI7.Locked=true
PI7.Signal=SAI2_FS_A
PI8.GPIOParameters=GPIO_Label
PI8.GPIO_Label=NC1 [TP2]
PI8.Locked=true
PI8.Signal=RTC_TS
PI9.GPIOParameters=GPIO_Label
PI9.GPIO_Label=LCD_VSYNC [RK043FN48H-CT672B_VSYNC]
PI9.Locked=true
PI9.Mode=RGB565
PI9.Signal=LTDC_VSYNC
PJ0.GPIOParameters=GPIO_Label
PJ0.GPIO_Label=LCD_R1 [RK043FN48H-CT672B_R1]
PJ0.Locked=true
PJ0.Signal=LTDC_R1
PJ1.GPIOParameters=GPIO_Label
PJ1.GPIO_Label=LCD_R2 [RK043FN48H-CT672B_R2]
PJ1.Locked=true
PJ1.Signal=LTDC_R2
PJ10.GPIOParameters=GPIO_Label
PJ10.GPIO_Label=LCD_G3 [RK043FN48H-CT672B_G3]
PJ10.Locked=true
PJ10.Mode=RGB565
PJ10.Signal=LTDC_G3
PJ11.GPIOParameters=GPIO_Label
PJ11.GPIO_Label=LCD_G4 [RK043FN48H-CT672B_G4]
PJ11.Locked=true
PJ11.Mode=RGB565
PJ11.Signal=LTDC_G4
PJ12.GPIOParameters=GPIO_Label
PJ12.GPIO_Label=OTG_FS_VBUS
PJ12.Locked=true
PJ12.Signal=GPIO_Input
PJ13.GPIOParameters=GPIO_Label
PJ13.GPIO_Label=LCD_B1 [RK043FN48H-CT672B_B1]
PJ13.Locked=true
PJ13.Signal=LTDC_B1
PJ14.GPIOParameters=GPIO_Label
PJ14.GPIO_Label=LCD_B2 [RK043FN48H-CT672B_B2]
PJ14.Locked=true
PJ14.Signal=LTDC_B2
PJ15.GPIOParameters=GPIO_Label
PJ15.GPIO_Label=LCD_B3 [RK043FN48H-CT672B_B3]
PJ15.Locked=true
PJ15.Mode=RGB565
PJ15.Signal=LTDC_B3
PJ2.GPIOParameters=GPIO_Label
PJ2.GPIO_Label=LCD_R3 [RK043FN48H-CT672B_R3]
PJ2.Locked=true
PJ2.Mode=RGB565
PJ2.Signal=LTDC_R3
PJ3.GPIOParameters=GPIO_Label
PJ3.GPIO_Label=LCD_R4 [RK043FN48H-CT672B_R4]
PJ3.Locked=true
PJ3.Mode=RGB565
PJ3.Signal=LTDC_R4
PJ4.GPIOParameters=GPIO_Label
PJ4.GPIO_Label=LCD_R5 [RK043FN48H-CT672B_R5]
PJ4.Locked=true
PJ4.Mode=RGB565
PJ4.Signal=LTDC_R5
PJ5.GPIOParameters=GPIO_Label
PJ5.GPIO_Label=LCD_R6 [RK043FN48H-CT672B_R6]
PJ5.Locked=true
PJ5.Mode=RGB565
PJ5.Signal=LTDC_R6
PJ6.GPIOParameters=GPIO_Label
PJ6.GPIO_Label=LCD_R7 [RK043FN48H-CT672B_R7]
PJ6.Locked=true
PJ6.Mode=RGB565
PJ6.Signal=LTDC_R7
PJ7.GPIOParameters=GPIO_Label
PJ7.GPIO_Label=LCD_G0 [RK043FN48H-CT672B_G0]
PJ7.Locked=true
PJ7.Signal=LTDC_G0
PJ8.GPIOParameters=GPIO_Label
PJ8.GPIO_Label=LCD_G1 [RK043FN48H-CT672B_G1]
PJ8.Locked=true
PJ8.Signal=LTDC_G1
PJ9.GPIOParameters=GPIO_Label
PJ9.GPIO_Label=LCD_G2 [RK043FN48H-CT672B_G2]
PJ9.Locked=true
PJ9.Mode=RGB565
PJ9.Signal=LTDC_G2
PK0.GPIOParameters=GPIO_Label
PK0.GPIO_Label=LCD_G5 [RK043FN48H-CT672B_G5]
PK0.Locked=true
PK0.Mode=RGB565
PK0.Signal=LTDC_G5
PK1.GPIOParameters=GPIO_Label
PK1.GPIO_Label=LCD_G6 [RK043FN48H-CT672B_G6]
PK1.Locked=true
PK1.Mode=RGB565
PK1.Signal=LTDC_G6
PK2.GPIOParameters=GPIO_Label
PK2.GPIO_Label=LCD_G7 [RK043FN48H-CT672B_G7]
PK2.Locked=true
PK2.Mode=RGB565
PK2.Signal=LTDC_G7
PK3.GPIOParameters=GPIO_Speed,PinState,GPIO_Label
PK3.GPIO_Label=LCD_BL_CTRL [STLD40DPUR_EN]
PK3.GPIO_Speed=GPIO_SPEED_FREQ_LOW
PK3.Locked=true
PK3.PinState=GPIO_PIN_SET
PK3.Signal=GPIO_Output
PK4.GPIOParameters=GPIO_Label
PK4.GPIO_Label=LCD_B5 [RK043FN48H-CT672B_B5]
PK4.Locked=true
PK4.Mode=RGB565
PK4.Signal=LTDC_B5
PK5.GPIOParameters=GPIO_Label
PK5.GPIO_Label=LCD_B6 [RK043FN48H-CT672B_B6]
PK5.Locked=true
PK5.Mode=RGB565
PK5.Signal=LTDC_B6
PK6.GPIOParameters=GPIO_Label
PK6.GPIO_Label=LCD_B7 [RK043FN48H-CT672B_B7]
PK6.Locked=true
PK6.Mode=RGB565
PK6.Signal=LTDC_B7
PK7.GPIOParameters=GPIO_Label
PK7.GPIO_Label=LCD_DE [RK043FN48H-CT672B_DE]
PK7.Locked=true
PK7.Mode=RGB565
PK7.Signal=LTDC_DE
PinOutPanel.CurrentBGAView=Top
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F746NGHx
ProjectManager.FirmwarePackage=STM32Cube FW_F7 V1.16.0
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0xA00
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=STM32CubeIDE
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=STM32F746G_DISCO.ioc
ProjectManager.ProjectName=STM32F746G_DISCO
ProjectManager.StackSize=0xA00
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=false
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-HAL-true,2-SystemClock_Config-RCC-false-HAL-false,3-MX_CRC_Init-CRC-false-HAL-true,4-MX_QUADSPI_Init-QUADSPI-false-HAL-true,5-MX_DMA2D_Init-DMA2D-false-HAL-true,6-MX_FMC_Init-FMC-false-HAL-true,7-MX_LTDC_Init-LTDC-false-HAL-true,8-MX_I2C3_Init-I2C3-false-HAL-true,9-MX_TouchGFX_Init-STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0-false-HAL-false,10-MX_TouchGFX_Process-STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0-false-HAL-false,0-MX_CORTEX_M7_Init-CORTEX_M7-false-HAL-true
QUADSPI.ChipSelectHighTime=QSPI_CS_HIGH_TIME_6_CYCLE
QUADSPI.ClockPrescaler=1
QUADSPI.FifoThreshold=4
QUADSPI.FlashSize=24
QUADSPI.IPParameters=ClockPrescaler,FifoThreshold,SampleShifting,FlashSize,ChipSelectHighTime
QUADSPI.SampleShifting=QSPI_SAMPLE_SHIFTING_HALFCYCLE
RCC.AHBFreq_Value=200000000
RCC.APB1CLKDivider=RCC_HCLK_DIV4
RCC.APB1Freq_Value=50000000
RCC.APB1TimFreq_Value=100000000
RCC.APB2CLKDivider=RCC_HCLK_DIV2
RCC.APB2Freq_Value=100000000
RCC.APB2TimFreq_Value=200000000
RCC.CECFreq_Value=32786.88524590164
RCC.CortexFreq_Value=200000000
RCC.EthernetFreq_Value=200000000
RCC.FCLKCortexFreq_Value=200000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=200000000
RCC.HSE_VALUE=25000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=50000000
RCC.I2C2Freq_Value=50000000
RCC.I2C3Freq_Value=50000000
RCC.I2C4Freq_Value=50000000
RCC.I2SFreq_Value=50000000
RCC.IPParameters=AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,CECFreq_Value,CortexFreq_Value,EthernetFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2C4Freq_Value,I2SFreq_Value,LCDTFToutputFreq_Value,LPTIM1Freq_Value,LSE_VALUE,LSI_VALUE,MCO2PinFreq_Value,PLL48CLockSelection,PLLCLKFreq_Value,PLLI2SN,PLLI2SPCLKFreq_Value,PLLI2SQCLKFreq_Value,PLLI2SRCLKFreq_Value,PLLI2SRoutputFreq_Value,PLLM,PLLN,PLLQ,PLLQCLKFreq_Value,PLLQoutputFreq_Value,PLLSAIN,PLLSAIP,PLLSAIPCLKFreq_Value,PLLSAIQCLKFreq_Value,PLLSAIR,PLLSAIRCLKFreq_Value,PLLSAIRDiv,PLLSAIoutputFreq_Value,PLLSourceVirtual,RNGFreq_Value,SAI1Freq_Value,SAI2Freq_Value,SDMMCClockSelection,SDMMCFreq_Value,SPDIFRXFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5Freq_Value,UART7Freq_Value,UART8Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USART6Freq_Value,USBFreq_Value,VCOI2SOutputFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAIOutputFreq_Value
RCC.LCDTFToutputFreq_Value=9600000
RCC.LPTIM1Freq_Value=50000000
RCC.LSE_VALUE=32768
RCC.LSI_VALUE=32000
RCC.MCO2PinFreq_Value=200000000
RCC.PLL48CLockSelection=RCC_CLK48SOURCE_PLLSAIP
RCC.PLLCLKFreq_Value=200000000
RCC.PLLI2SN=100
RCC.PLLI2SPCLKFreq_Value=50000000
RCC.PLLI2SQCLKFreq_Value=50000000
RCC.PLLI2SRCLKFreq_Value=50000000
RCC.PLLI2SRoutputFreq_Value=50000000
RCC.PLLM=25
RCC.PLLN=400
RCC.PLLQ=9
RCC.PLLQCLKFreq_Value=44444444.44444445
RCC.PLLQoutputFreq_Value=44444444.44444445
RCC.PLLSAIN=384
RCC.PLLSAIP=RCC_PLLSAIP_DIV8
RCC.PLLSAIPCLKFreq_Value=48000000
RCC.PLLSAIQCLKFreq_Value=192000000
RCC.PLLSAIR=5
RCC.PLLSAIRCLKFreq_Value=76800000
RCC.PLLSAIRDiv=RCC_PLLSAIDIVR_8
RCC.PLLSAIoutputFreq_Value=48000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.RNGFreq_Value=48000000
RCC.SAI1Freq_Value=192000000
RCC.SAI2Freq_Value=192000000
RCC.SDMMCClockSelection=RCC_SDMMC1CLKSOURCE_CLK48
RCC.SDMMCFreq_Value=48000000
RCC.SPDIFRXFreq_Value=50000000
RCC.SYSCLKFreq_VALUE=200000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=50000000
RCC.UART5Freq_Value=50000000
RCC.UART7Freq_Value=50000000
RCC.UART8Freq_Value=50000000
RCC.USART1Freq_Value=100000000
RCC.USART2Freq_Value=50000000
RCC.USART3Freq_Value=50000000
RCC.USART6Freq_Value=100000000
RCC.USBFreq_Value=48000000
RCC.VCOI2SOutputFreq_Value=100000000
RCC.VCOInputFreq_Value=1000000
RCC.VCOOutputFreq_Value=400000000
RCC.VCOSAIOutputFreq_Value=384000000
SH.ADCx_IN0.0=ADC3_IN0
SH.ADCx_IN0.ConfNb=1
SH.FMC_A0.0=FMC_A0,12b-sda1
SH.FMC_A0.ConfNb=1
SH.FMC_A1.0=FMC_A1,12b-sda1
SH.FMC_A1.ConfNb=1
SH.FMC_A10.0=FMC_A10,12b-sda1
SH.FMC_A10.ConfNb=1
SH.FMC_A11.0=FMC_A11,12b-sda1
SH.FMC_A11.ConfNb=1
SH.FMC_A14_BA0.0=FMC_BA0,FourSdramBanks1
SH.FMC_A14_BA0.ConfNb=1
SH.FMC_A15_BA1.0=FMC_BA1,FourSdramBanks1
SH.FMC_A15_BA1.ConfNb=1
SH.FMC_A2.0=FMC_A2,12b-sda1
SH.FMC_A2.ConfNb=1
SH.FMC_A3.0=FMC_A3,12b-sda1
SH.FMC_A3.ConfNb=1
SH.FMC_A4.0=FMC_A4,12b-sda1
SH.FMC_A4.ConfNb=1
SH.FMC_A5.0=FMC_A5,12b-sda1
SH.FMC_A5.ConfNb=1
SH.FMC_A6.0=FMC_A6,12b-sda1
SH.FMC_A6.ConfNb=1
SH.FMC_A7.0=FMC_A7,12b-sda1
SH.FMC_A7.ConfNb=1
SH.FMC_A8.0=FMC_A8,12b-sda1
SH.FMC_A8.ConfNb=1
SH.FMC_A9.0=FMC_A9,12b-sda1
SH.FMC_A9.ConfNb=1
SH.FMC_D0_DA0.0=FMC_D0,sd-16b-d1
SH.FMC_D0_DA0.ConfNb=1
SH.FMC_D10_DA10.0=FMC_D10,sd-16b-d1
SH.FMC_D10_DA10.ConfNb=1
SH.FMC_D11_DA11.0=FMC_D11,sd-16b-d1
SH.FMC_D11_DA11.ConfNb=1
SH.FMC_D12_DA12.0=FMC_D12,sd-16b-d1
SH.FMC_D12_DA12.ConfNb=1
SH.FMC_D13_DA13.0=FMC_D13,sd-16b-d1
SH.FMC_D13_DA13.ConfNb=1
SH.FMC_D14_DA14.0=FMC_D14,sd-16b-d1
SH.FMC_D14_DA14.ConfNb=1
SH.FMC_D15_DA15.0=FMC_D15,sd-16b-d1
SH.FMC_D15_DA15.ConfNb=1
SH.FMC_D1_DA1.0=FMC_D1,sd-16b-d1
SH.FMC_D1_DA1.ConfNb=1
SH.FMC_D2_DA2.0=FMC_D2,sd-16b-d1
SH.FMC_D2_DA2.ConfNb=1
SH.FMC_D3_DA3.0=FMC_D3,sd-16b-d1
SH.FMC_D3_DA3.ConfNb=1
SH.FMC_D4_DA4.0=FMC_D4,sd-16b-d1
SH.FMC_D4_DA4.ConfNb=1
SH.FMC_D5_DA5.0=FMC_D5,sd-16b-d1
SH.FMC_D5_DA5.ConfNb=1
SH.FMC_D6_DA6.0=FMC_D6,sd-16b-d1
SH.FMC_D6_DA6.ConfNb=1
SH.FMC_D7_DA7.0=FMC_D7,sd-16b-d1
SH.FMC_D7_DA7.ConfNb=1
SH.FMC_D8_DA8.0=FMC_D8,sd-16b-d1
SH.FMC_D8_DA8.ConfNb=1
SH.FMC_D9_DA9.0=FMC_D9,sd-16b-d1
SH.FMC_D9_DA9.ConfNb=1
SH.FMC_NBL0.0=FMC_NBL0,Sd2ByteEnable1
SH.FMC_NBL0.ConfNb=1
SH.FMC_NBL1.0=FMC_NBL1,Sd2ByteEnable1
SH.FMC_NBL1.ConfNb=1
SH.FMC_SDCLK.0=FMC_SDCLK,12b-sda1
SH.FMC_SDCLK.ConfNb=1
SH.FMC_SDNCAS.0=FMC_SDNCAS,12b-sda1
SH.FMC_SDNCAS.ConfNb=1
SH.FMC_SDNRAS.0=FMC_SDNRAS,12b-sda1
SH.FMC_SDNRAS.ConfNb=1
SH.FMC_SDNWE.0=FMC_SDNWE,12b-sda1
SH.FMC_SDNWE.ConfNb=1
SH.GPXTI13.0=GPIO_EXTI13
SH.GPXTI13.ConfNb=1
SH.GPXTI6.0=GPIO_EXTI6
SH.GPXTI6.ConfNb=1
SH.S_TIM12_CH1.0=TIM12_CH1
SH.S_TIM12_CH1.ConfNb=1
SH.S_TIM1_CH1.0=TIM1_CH1
SH.S_TIM1_CH1.ConfNb=1
SH.S_TIM2_CH1_ETR.0=TIM2_CH1
SH.S_TIM2_CH1_ETR.ConfNb=1
SH.S_TIM3_CH1.0=TIM3_CH1
SH.S_TIM3_CH1.ConfNb=1
SH.S_TIM5_CH4.0=TIM5_CH4
SH.S_TIM5_CH4.ConfNb=1
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.ApplicationCcGraphicsJjApplication=TouchGFXOoGenerator
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.GraphicsJjApplication_Checked=true
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.IPParameters=ApplicationCcGraphicsJjApplication,tgfx_hardware_accelerator,tgfx_display_interface,tgfx_vsync,tgfx_buffering_strategy,tgfx_location,tgfx_address1,tgfx_pixel_format,tgfx_address2
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.tgfx_address1=0xC0000000
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.tgfx_address2=0xC003FC00
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.tgfx_buffering_strategy=Double
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.tgfx_display_interface=disp_ltdc
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.tgfx_hardware_accelerator=dma_2d
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.tgfx_location=By Address
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.tgfx_pixel_format=RGB565\:16
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0.tgfx_vsync=vsync_ltdc
STMicroelectronics.X-CUBE-TOUCHGFX.4.13.0_SwParameter=ApplicationCcGraphicsJjApplication\:TouchGFXOoGenerator;
VP_CRC_VS_CRC.Mode=CRC_Activate
VP_CRC_VS_CRC.Signal=CRC_VS_CRC
VP_DMA2D_VS_DMA2D.Mode=DMA2D_Activate
VP_DMA2D_VS_DMA2D.Signal=DMA2D_VS_DMA2D
VP_FREERTOS_VS_CMSIS_V1.Mode=CMSIS_V1
VP_FREERTOS_VS_CMSIS_V1.Signal=FREERTOS_VS_CMSIS_V1
VP_STMicroelectronics.X-CUBE-TOUCHGFX_VS_GraphicsJjApplication_4.13.0.Mode=GraphicsJjApplication
VP_STMicroelectronics.X-CUBE-TOUCHGFX_VS_GraphicsJjApplication_4.13.0.Signal=STMicroelectronics.X-CUBE-TOUCHGFX_VS_GraphicsJjApplication_4.13.0
VP_SYS_VS_tim6.Mode=TIM6
VP_SYS_VS_tim6.Signal=SYS_VS_tim6
board=32F746GDISCOVERY
boardIOC=true
